Unit 	Energy efficiency in thermal and electrical processes and horizontal utilities	
Stage	Stage 2: Implementation / Middle Manager	
Program	This is the fourth training unit. This unit shall focus at the roles of the employees regarding identification for energy efficiency measures in thermal processes and electrical processes and horizontal utilities.	
Planning	Target group category:		Top management (Executives or their representatives)	
		x	Middle management (Energy manager)	
			General employees (Operators of the machines)	
	Specific group:	Lower technical management and general employees	
	No of participants:	Up to 10 participants.	
	Duration:	2 hours	
	Elements:	Roundtable to identify energy management measures in thermal and electrical processes and horizontal utilities in their facilities.	
General objectives	Aim: 	Middle managers shall recognise Energy efficiency as an important company target, learn different difficulties to identify energy efficiency measures and implement them.	
	Verification:	Conclusion with a set of multiple-choice questions	
Specific objectives	Aim: 		a)	Know breakdown energy in company
b)	Understanding what it is possible to save energy in the company.
c)	Explain how it is possible to save energy according to different type of installations.	
	Verification: 		Conclusion with a set of multiple-choice questions	
Concept	Type of material:	Presentation, pin Board, and material to develop a round table.	
	Contribution:	Develop skills and knowledge related to thermal processes, in electrical processes and horizontal utilities existing in their facilities. 
Recognize difficulties to identify energy efficient in all levels of organization and how middle managers could help to reduce energy consumption.	
	Training levels:	Understand: contents/methods thermal processes, in electrical processes and horizontal utilities.
Apply: Define any idea based on concepts learning in a previous stage
Evaluate: Prioritizing different ideas considering different criteria analysed in a first stage.	
Learning activities	The training session is based on slides in a first stage, where it will be explained main characteristics in energy efficiency in thermal processes, in electrical processes and horizontal utilities existing in their facilities. 
Then it will be developed a roundtable where participants will give ideas to implement energy efficiency measurements in their company, and criteria to consider to implemented them.	
Learning method	x	Master class		Case studies		Diagnostic analysis	
	x	Discussion forum		Self-learning		Problem-based learning	
		Role play	x	Cooperative learning	x	Others	
Learning resources	Trainer:	Training slides 
Flipchart
Pin board 
Methodology.	
	Participants:	Pen and paper.	

Evaluation Test
1.	Depending on the heat exchanger device, boilers can be classified into:
a.	Water pipe and gas pipe.
b.	Standard, Low temperature and condensation.
c.	  Watertight and airtight
2.	How is the performance of a boiler calculated?
a.	Performance (%) = 100 - losses
b.	Performance (%) = 100 x losses
c.	  Performance (%) = 100 / losses
3.	What parameters can’t be measured with the gas analyzer?
a.	  Excess of air
b.	Heated water temperature.
c.	  Flue gas temperature
4.	When looking at cold production, it is necessary to evaluate the improvement measures in:
a.	  Cooling cycle (devices)
b.	Walls and surfaces of cooling chambers.
c.	  Both
5.	Which is not a good measure in Temperature Control in Air Conditioning Installations?
a.	  Installation of temperature control systems (thermostats).
b.	Creating the On/Off protocol
c.	  Always provide the same temperature.
6.	What are the opportunities to save energy in electric engines?
a.	Adapting the power of electric motors to real requirements
b.	Increase the power by 10% over the design device.
c.	  Adapt the selected engine power to the nearest standard.
7.	¿What is luminous efficiency?
a.	Relationship between the luminous flux (lumens) and the area.
b.	It is the ratio of luminous flux to power (usually electric power.
c.	  The measure of the power of electromagnetic radiation related to visible light.
8.	¿What is a recommendation for the energy efficiency of compressed air systems?
a.	  Design a united distribution network.
b.	Set a higher working pressure than necessary.
c.	  Install recovery system heat.
9.	How can you use a thermal imaging camera?
a.	  To detect termites and humidity.
b.	To detect condensation and filtering
c.	  For all of them